<?xml version="1.0" encoding="UTF-8"?>
<Network xmlns="http://www.xmos.com" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:schemaLocation="http://www.xmos.com http://www.xmos.com" ManuallySpecifiedRouting="true">
  <Type>Board</Type>
  <Name>xCORE-200 MC Audio</Name>
  <Declarations>
    <Declaration>tileref tile[2]</Declaration>
    <Declaration>tileref usb_tile</Declaration>
  </Declarations>
  <Packages>
    <Package id="0" Type="XS2-UEnA-512-FB236">
      <Nodes>
        <Node Id="0" InPackageId="0" Type="XS2-L16A-512" OscillatorSrc="1" SystemFrequency="500MHz">
          <Boot>
            <Source Location="bootFlash"/>
          </Boot>
          <Tile Number="0" Reference="tile[0]">
            <Port Location="XS1_PORT_1B" Name="PORT_SQI_CS"/>
            <Port Location="XS1_PORT_1C" Name="PORT_SQI_SCLK"/>
            <Port Location="XS1_PORT_4B" Name="PORT_SQI_SIO"/>
          </Tile>
          <Tile Number="1" Reference="tile[1]"/>
        </Node>
        <Node Id="1" InPackageId="1" Type="periph:XS1-SU" Reference="usb_tile" Oscillator="24MHz">
        </Node>
      </Nodes>
      <Links>
        <Link Encoding="5wire">
          <LinkEndpoint NodeId="0" Link="8" Delays="52clk,52clk"/>
          <LinkEndpoint NodeId="1" Link="0" Delays="1clk,1clk"/>
        </Link>
      </Links>
    </Package>
  </Packages>
  <Nodes>
    <Node Id="2" Type="device:" RoutingId="0x8000">
      <Service Id="0" Proto="xscope_host_data(chanend c);">
        <Chanend Identifier="c" end="3"/>
      </Service>
    </Node>
  </Nodes>
  <Links>
    <Link Encoding="2wire" Delays="4,4" Flags="XSCOPE">
      <LinkEndpoint NodeId="0" Link="0"/>
      <LinkEndpoint NodeId="2" Chanend="1"/>
    </Link>
  </Links>
  <ExternalDevices>
    <Device NodeId="0" Tile="0" Class="SQIFlash" Name="bootFlash" Type="S25FL116K" PageSize="256" SectorSize="4096" NumPages="8192">
      <Attribute Name="PORT_SQI_CS" Value="PORT_SQI_CS"/>
      <Attribute Name="PORT_SQI_SCLK"   Value="PORT_SQI_SCLK"/>
      <Attribute Name="PORT_SQI_SIO"  Value="PORT_SQI_SIO"/>
    </Device>
  </ExternalDevices>
  <JTAGChain>
    <JTAGDevice NodeId="0"/>
  </JTAGChain>
</Network>
